A screenshot of a video game

Description automatically generatedA screen shot of a video game

Description automatically generated

A screen shot of a video game

Description automatically generated

Questions:

- ask about routing with ground and power plane with via ?

- pad properties

- holes - do I need to set the net to anything or do anything?

- Thickness/layer recommendation (1.5 with standard format)

- silk to solder mask clearance (mine is 9.4mil) changed from 10mil to 7.5mil

- hole size constraint (changed from 100mil to 130mil)

Graphical user interface, application

Description automatically generatedA circuit board

Description automatically generated